Running APRS+SA for the first time:  The minimal settings required to configure APRS+SA on a Single Port TNC
1) Unzip the APRS+SA file to its own directory
2) Run Setup.exe
3) Start APRS+SA by executing APRSPLUS.EXE - you will get a notification that you are running an unregistered copy of APRS+SA.
4) Click the Setup menu, select Main.
5) Enter your Callsign
6) Enter you Latitude - use decimal degrees for quick start
7) Enter your Longitude - use decimal degrees for quick start
8) Select a TNC Configuration File
9) Check your Unproto path, default is WIDE,WIDE. 
10) Configure Port 1, the TNC port. 
	a) Set Baud Rate.
	b) Click the Port, and select the appropriate Com Port to Open the serial port. 
	You should see configuration data on the TNC page of the main program window.

You can close the Setup window and reopen at any time, it if you wish.

At this point, if your station is on an active RF network, and radio and TNC are on, you should begin to see data coming in on the TNC.

Start Street Atlas.  Then from the APRS+SA main window, press the keys,  Ctrl-2.  This will draw the position of all known station.  